

# Pre-Backfill Inspection Checklist

**\*Before calling for your inspection, please make sure the following items are complete:**

**O** Township stamped plans are onsite.

**O** All debris, rubbish, rocks etc. removed from area to be backfilled.

**O** Temporary bracing, and/or floor deck is installed.

**O** Cold room/crawlspace ventilation is installed.

**O** Perimeter insulation is complete (if required).

**O** Damp-proofing/parging for concrete block is complete.

**O** The top cores of concrete block are filled with concrete/anchor bolts.

**O** ‘Dimple board’ or other backfill protection material is installed.

**O** Membrane/waterproofing is installed on ICF and extends onto the footing.

**O** Weeping tile is installed, including any window well drains, 4” minimum.

**O** Weeping tile extends away from the foundation and is supported.

**O** Minimum of 6” of clear stone is installed over weeping tile.

**O** Landscape fabric, silt cloth or ‘socked’ weeping tile is complete.

**O** Any field reviews or soils reports from Engineers are received.

# When you have checked all applicable boxes, please email building@swox.org to book your inspection.

**We will perform the inspection within 2 business days.**