

# Plumbing Above Ground Inspection Checklist

**\*Before calling for your inspection, please make sure the following items are complete:**

**O** Township stamped plans are onsite.

**O** Cleanouts are installed at the base of stacks/changes in direction.

**O** Drainage pipe is sloped to a minimum of 1 in 50, max. 1 in 25.

**O** Drain water heat recovery unit (DWHR) is installed (year-round homes).

**O** Drain and vent pipes are supported/clamped every 4 ft. min.

**O** Drain and vent pipes are capped/ charged with air to 5 psi for 15 mins. OR capped and filled with water for 15 minutes with a min. 10’ column

**O** Waterlines are capped and airtested to 100 psi for 2 hrs. min.

**O** Waterlines have clips/clamps installed max. 1m/ 3’3” apart.

**O** Vents are a minimum of 3” size where they exit the roof or building. **O** Vents are sloped properly and secured to framing at the building exit. **O** Incoming water supply line is ¾” minimum in size. (if installed)

**O** Basement sewage ejector is installed/vented (2” min. vent size)

**O** Protection plates are installed where pipes are drilled through studs and top/bottom plates where penetration by screws/nails is possible.

# When you have checked all applicable boxes, please

**email** [**building@swox.org**](mailto:building@swox.org%20) **to book your inspection.**

# We will perform the inspection within 2 business days.