

# Footing Inspection Checklist

**\*Before calling for your inspection, please make sure the following items are complete:**

**O** Township stamped plans are onsite.

**O** Building size and position as per the site plan.

**O** Soil is compacted, engineered fill placed (if required)

**O** Engineering report submitted (if required)

**O** Excavated down to undisturbed soil or bedrock.

**O** Pinning to bedrock complete .

**O** Footing forms are constructed as per the foundation plan.

**O** Stepped footings are constructed (max.rise 24”, minimum run 24”)

**O** Piers and strip footings are sized and constructed as per plan.

**O** Frost protection, under-slab insulation installed and taped. **O** Re-bar, wire mesh and all other reinforcement is installed. **O** Underslab moisture barrier (poly) is installed (if required)

**O** Forms are free from water, debris, organic and/or frozen material.

**O** Dowels into existing concrete or vertical bedrock are installed.

**O** Deck footings are positioned and sized correctly and complete. **O** Tarps, heaters etc. are onsite if pouring in cold weather.

# When you have checked all applicable boxes, please email [building@swox.org](mailto:building@swox.org%20) to book your inspection.

**We will perform the inspection within 2 business days.**